Contract No. PGC-95-12-01


TECHNICAL SPECIFICATION SECTION 6 – PLUGGING THE OIL WELL
6.1 – SCOPE 

The work included in this section consists of plugging the oil well completely with cement, venting the well casings if necessary, collecting and disposing of well fluids if necessary and installing a permanent marker at the well.
6.2 – PROCEDURE
A. General – The oil well plugging operations shall conform to the applicable requirements of Chapter 78 of the PA Code; specifically sections 78.91 to 78.98 of Chapter 78.  The PGC does not have any information on the total depth, diameter, casings, subsurface strata or condition of the well.  Therefore, the well shall be plugged full depth with cement according to Section 78.91h of Chapter 78.
B. Plugging the Well – The Contractor shall deliver and set up all equipment and materials at the oil well for plugging operations.  Remove portions of the well head to allow for plugging operations.  Install pumping equipment in the well.  Cement the well from the attainable bottom up for the total depth of the well.  Maintain accurate records of the quantity per sack (94-pound) of Portland cement used in the well plugging operations.  After plugging operations are complete, cut off and remove the well casing at least 18-inches below the ground surface.  
C. Fluid Containment – Provide an earthen berm around the oil well to capture any fluids which may discharge from the casing during well plugging operations.  Provide absorbent materials if necessary to prevent fluids from leaving the containment area.  Dispose of fluid soaked materials if necessary.  It is not known if there will be substantial amounts of oil to dispose of during this project.  Collection and disposal of minor amounts of oil and absorbent materials will be considered incidental to the overall project costs and no separate payment will be processed.  If there are substantial amounts of oil to be disposed of which would cause an undo financial hardship to the Contractor, a change order will be processed to provide for proper disposal of the oil and protection of the environment.
D. Final Grading – Restore the area around the wells to the approximate original ground surface.  Minor amounts of oil are allowed to be worked into the soil around the wells.  Conduct site restoration operations according to Section 9 of these Technical Specifications after the permanent markers are in place. 
E. Permanent Markers – Upon completion of plugging the well, install a permanent marker of concrete, metal, plastic or an equally durable material.  The permanent marker shall conform to the requirements of Section 78.96 of Chapter 78.
6.3 – MEAUSREMENT AND PAYMENT
Sack (94-pound) of cement for the well plugging.  No separate measurement or payment for pumping or additives related to cement plugging operations.  No separate measurement or payment for venting, permanent marking of the well and collection and disposal of fluids.  
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